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Fax: (269) 381-3455
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Wellspring Litter

Product Guide Specification

Specifier Notes:  This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, including MasterFormat, SectionFormat, and PageFormat, as described in The Project Resource Manual—CSI Manual of Practice, Fifth Edition.
The section must be carefully reviewed and edited by the Architect to meet the requirements of the project and local building code.  Coordinate this section with other specification sections and the Drawings.  Delete all “Specifier Notes” after editing this section.

Section numbers are from MasterFormat 2010 Edition.
SECTION 12 93 23       TRASH AND LITTER RECEPTORS
Specifier Notes:  This section covers Landscape Forms, Inc. “Wellspring TM” litter/recycle receptacles.  Consult Landscape Forms, Inc. for assistance in editing this section for the specific application.

PART 1
GENERAL

1.1
SECTION INCLUDES
A.
Litter receptacles.
1.2
REFERENCES
Specifier Notes:  List standards referenced in this section, complete with designations and titles.  This article does not require compliance with standards, but is merely a listing of those used.

A.
ASTM Testing Standards: 
1.
ASTM B 117 – Standard Practice for Operating Salt Spray (Fog) Apparatus.

2.
ASTM D 522 – Standard Test Methods for Mandrel Bend Test of Attached Organic Coatings.

3.
ASTM D 523 – Standard Test Method for Specular Gloss.
4.
ASTM D 2247 – Standard Practice for Testing Water Resistance of Coatings in 100% Relative Humidity.

5.
ASTM D 2794 – Standard Test Method for Resistance of Organic Coatings to the Effects of Rapid Deformation (Impact).

6.
ASTM D 3359 – Standard Test Methods for Measuring Adhesion by Tape Test.

7.
ASTM D 3363 – Standard Test Method for Film Hardness by Pencil Test.

8.
ASTM G 155 – Standard Practice for Operating Xenon Arc Light Apparatus for Exposure of Non-Metallic Materials.
B.
ISO Testing Standards:
1.
ISO 1520 – Paints and Varnishes – Cupping Test.

2.
ISO 2815 – Paints and Varnishes – Buchholz Indentation Test.
1.3
SUBMITTALS
A.
Product Data: Submit manufacturer’s product data, storage and handling requirements and recommendations, installation methods and available colors, styles, patterns and textures. 

B.
Shop Drawings: Submit manufacturer’s shop drawings, including plans and elevations, indicating overall dimensions.
C.
Samples:  Submit manufacturer’s samples of materials, finishes, and colors.
D.
Warranty: Manufacturer’s standard warranty.
1.4
QUALITY ASSURANCE
A.
Manufacturer’s Qualifications: Manufacturer regularly engaged in manufacture of site furnishings since 1969.
B.
Product Support: Products are supported with complete engineering drawings and design patents.

C.
Base Worth: An installed base of products worth in excess of one hundred million dollars.

D.
Assets: Excess of twenty million dollars in assets.

E.
Production: Orders are filled within a 40-day schedule.

F.
Facility Operator: Welders and machine operators are certified.
1.5
DELIVERY, STORAGE, AND HANDLING
A.
Delivery:  Deliver materials to site in manufacturer’s original, unopened containers and packaging, with labels clearly identifying product name and manufacturer.

B.
Storage: Store materials in clean, dry area in accordance with manufacturer’s instructions.  Keep materials in manufacturer’s original, unopened containers and packaging until installation.
C.
Handling:  Protect materials and finish during handling and installation to prevent damage.

1.6
WARRANTY
A.
Warranty Information:  

-Products will be free from defects in material and/or workmanship for a period of three years from the date of invoice.

-The warranty does not apply to damage resulting from accident, alteration, misuse, tampering, negligence, or abuse.

- Landscape Forms, Inc. shall, at its option, repair, replace, or refund the purchase price of any items found defective upon inspection by an authorized Landscape Forms service representative.
-Purchasers should be aware that normal use of these high quality products can result in superficial damage affecting the finish.  Scratches, nicks, and dents are to be considered normal wear and tear, and are not the responsibility of the manufacturer.
PART 2
PRODUCTS

2.1
MANUFACTURER
A.
Landscape Forms, Inc., 7800 E. Michigan Ave, Kalamazoo, Michigan 49048.                       Phone: (800) 521-2546. Fax (269) 381-3455.  Website www.landscapeforms.com                       E-mail:  specify@landscapeforms.com
2.2
TRASH AND LITTER RECEPTORS
A.
“Wellspring” Litter Receptacles
Specifier Notes:  Specify opening type of litter receptacles.
B.
Size: 
-Height: 31-1/2 inches.

-Body: 22-1/2 inches square.

C.
Opening:

1.  Side Opening

Specifier Notes:  Specify litter receptacle mounting.

D.
Mounting: 
1.
Free Standing: Shipped with freestanding glides
2.
Surface Mounted
2.3
MATERIAL
A.
Litter Body: All wood construction, litter bodies are assembled with glued, mortise and tenon or doweled joints. All fasteners used for assembly are stainless steel type A tapping screws.  All exposed edges are eased.
B.
Litter Lid: 319 cast aluminum.
C.
Wood Selection: 

-Teak: Solid stock, select furniture grade hardwood, unfinished.
Specifier Notes:  Specify litter receptacle mounting material.
D.
Mounting:
1.
Surface Mount Bracket: Type 304 stainless steel with 3/8” diameter hole for anchor.

2.
Glides (Freestanding): Nylon tack style.
2.4
ACCESSORIES
Specifier Notes:  Specify anchor bolts for surface-mounted litter receptacles.  Delete for free-standing receptacles.
A.
Anchor Bolts:  Corrosion resistant recommended, not supplied by manufacturer.
2.5 RECYCLED CONTENT
A.
Litter Receptacle:
-Recyclable:  100 percent.

2.6
FABRICATION
A.
Shop assembled litter receptacles.
2.7
FINISHES
A.
Finish on Metal:  Landscape Forms, Inc. “Pangard II”.

1.
Primer:  Rust inhibitor 

2.
Topcoat:  Thermosetting TGIC polyester powder coat.  UV, chip, and flake resistant.
3.
Test Results:  “Pangard II”.

a.
Gloss Consistency, Gardner 60 Degrees, ASTM D 523:  Plus or minus 5 percent from standard.

b.
UV Resistance, Color and Gloss, ASTM G 155, Cycle 7:  Delta E less than 2 at 2.0 mils and less than 20 percent loss.

c.
Cross-Hatch Adhesion, ASTM D 3359, Method B:  100 percent pass.

d.
Flexibility Test, Mandrel, ASTM D 522:  3 mm at 2 mils.

e.
Erichsen Cupping, ISO 1520:  8 mm.

f.
Impression Hardness, Buchholz, ISO 2815:  95.

g.
Impact Test, ASTM D 2794:  60 inch-pounds at 2.5 mils.

h.
Pencil Hardness, ASTM D 3363:  2H minimum.

i.
Corrosion Resistance, 1,500-Hour Test, ASTM B 117: Max. undercutting 1 mm.

j.
Humidity Resistance, 1,500-Hour Test, ASTM D 2247:  Max. blisters 1 mm.

Specifier Notes:  Specify color of metal finish.  Consult Landscape Forms, Inc. for selection of standard colors and availability of custom colors.
4.
Color:  ____________ .

B.
Wood: Unfinished Teak
PART 3
EXECUTION

3.1
EXAMINATION
A.
Examine areas to receive litter receptacles.
B.
Notify Architect of conditions that would adversely affect installation or subsequent use.
C.
Do not begin installation until unacceptable conditions are corrected.

3.2
INSTALLATION
A.
Install litter receptacles in accordance with manufacturer’s instructions at locations indicated on the Drawings.

B.
Install litter receptacles level and plumb.
C.
Anchor litter receptacles securely in place.

3.3
ADJUSTING
A.
Finish Damage: Repair minor damages to finish in accordance with manufacturer’s instructions and as approved by Architect.
B.
Component Damage: Remove and replace damaged components that cannot be successfully repaired as determined by Architect.

3.4
CLEANING
A.
Clean litter receptacles promptly after installation in accordance with manufacturer’s instructions.

B.
Do not use harsh cleaning materials or methods that could damage finish.

3.5
PROTECTION
A.
Protect installed litter receptacles to ensure that, except for normal weathering, receptacles will be without damage or deterioration at time of Substantial Completion.
END OF SECTION


Landscape Forms
Wellspring Liter Receptacles

Page 4 of 4
06/15/2017

