IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2020-10-20T14:03:23"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.3.3.18 - Alternate UI 18.3.3.18"
Application: "Autodesk Revit 2018 (ENG)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENG)"

People and organizations
  Person "Mark.Conn" of Organization (no name given)
  Owner history of Person "Mark.Conn" of Organization (no name given) | application "Autodesk Revit 2018 (ENG)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENG)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "16Bike" | object type "16Bike" | names: "NBS_CyclepodsLtd_CrbStlCyclStnds_EasyliftPremiumDoubleSided:16Bike:9716" | material: materials ("NBS_CyclePodsLtd_Steel_Galvanized", "NBS_CyclepodsLtd_Polyethylene_MediumDensity_Red") | property sets: COBie

Types
  IFCBUILDINGELEMENTPROXYTYPE "16Bike" | USERDEFINED | 1 occurrence | material: materials ("NBS_CyclePodsLtd_Steel_Galvanized", "NBS_CyclepodsLtd_Polyethylene_MediumDensity_Red") | property sets: BOS_General, NBS_Data, Pset_FurnitureTypeCommon, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_40_30_21_12:Carbon steel cycle stands" (IFCTEXT)
    CodePerformance = "BS EN ISO 11461" (IFCTEXT)
    Color = "Red" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "A highly convenient gas-assisted two level bicycle parking system" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "5 + years" (IFCTEXT)
    Features = "Space saving, secure, compatible" (IFCTEXT)
    Finish = "Galvanised, galvanised and powder coated" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cyclepods.co.uk" (IFCTEXT)
    Material = "Aluminium track and Red polymer handle with steel support" (IFCTEXT)
    ModelNumber = "ELIFT01" (IFCTEXT)
    ModelReference = "EasyliftPremiumDoubleSided_16Bike" (IFCTEXT)
    Name = "CarbonSteelCycleStands_EasyliftPremiumDoubleSided_16Bike_CyclepodsLtd" (IFCTEXT)
    NominalWidth = 1945.0000029564 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "2900 x 2660 x 2100 x 1945 mm" (IFCTEXT)
    SustainabilityPerformance = "Frame and components made from widely recyclable materials" (IFCTEXT)
    WarrantyDescription = "5 years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CyclepodsLtd_CarbonSteelCycleStands_EasyliftPremiumDoubleSided_16Bike" (IFCTEXT)
    ManufacturerName = "Cyclepods Ltd" (IFCTEXT)
    ManufacturerURL = "https://www.cyclepods.co.uk/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/jmzuycfp" (IFCTEXT)
    NBSDescription = "Carbon steel cycle stands" (IFCTEXT)
    NBSReference = "45-35-86/301" (IFCTEXT)
    ProductInformation = "https://www.cyclepods.co.uk/easylift-premium/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_40_30_21_12" (IFCTEXT)
    Uniclass2015Title = "Carbon steel cycle stands" (IFCTEXT)
    Uniclass2015Version = "Products v1.15" (IFCTEXT)
    Version = "3" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    LoweringMechanism = "Gas assisted" (IFCTEXT)
    MinimumManoeuvringSpace = "2100 mm" (IFCTEXT)
    Security = "3 individual locking points per rack" (IFCTEXT)
  Pset_FurnitureTypeCommon | properties | on 1 type object
    IsBuiltIn = FALSE (IFCBOOLEAN)
    MainColor = "n/a" (IFCTEXT)
    NominalDepth = 2900.000004408 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 2660.0000040432 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 2100.000003192 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    Style = "Cycle stand" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcBuildingElementProxyType" (IFCTEXT)
    IfcExportType = "USERDEFINED" (IFCTEXT)