IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2020-07-10T11:24:01"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENG)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENG)"

People and organizations
  Person "Piotr.Bocian-NBS" of Organization (no name given)
  Owner history of Person "Piotr.Bocian-NBS" of Organization (no name given) | application "Autodesk Revit 2018 (ENG)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENG)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | object type "Level:Circle Head - Project Datum" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Minipod" | object type "NBS_CyclepodsLtd_PlstcsCyclLckrs_Minipod:Minipod" | names: "NBS_CyclepodsLtd_PlstcsCyclLckrs_Minipod:Minipod:304948" | material: materials ("NBS_CyclepodsLtd_StainlessSteel", "NBS_CyclepodsLtd_Plastic_Black") | property sets: BOS_General, NBS_Data, Pset_BuildingElementProxyCommon, IFC, COBie

Types
  IFCBUILDINGELEMENTPROXYTYPE "Minipod" | USERDEFINED | 1 occurrence | material: materials ("NBS_CyclepodsLtd_StainlessSteel", "NBS_CyclepodsLtd_Plastic_Black") | property sets: BOS_General, NBS_Data, Pset_BuildingElementProxyCommon, IFC, COBie

Property sets
  BOS_General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_CyclepodsLtd_PlasticsCycleLockers_Minipod" (IFCTEXT)
    ManufacturerName = "Cyclepods Ltd" (IFCTEXT)
    ManufacturerURL = "https:/​/​www.cyclepods.co.uk/​" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/bx2rfptm" (IFCTEXT)
    NBSDescription = "Plastics cycle lockers" (IFCTEXT)
    NBSReference = "45-35-86/313" (IFCTEXT)
    ProductInformation = "https://www.cyclepods.co.uk/minipod/" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_40_30_21_65" (IFCTEXT)
    Uniclass2015Title = "Plastics cycle lockers" (IFCTEXT)
    Uniclass2015Version = "Products v1.18" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    Colour = "Available in a range of different colours" (IFCTEXT)
    FinishAsDelivered = "Dimpled effect finish" (IFCTEXT)
    NumberOfStands = "16" (IFCTEXT)
    StandType = "Minipod Quadrant" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    FireRating = "n/a" (IFCTEXT)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    ThermalTransmittance = 0. (IFCREAL)
  IFC | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY) | on 1 type object
    IfcExportAs = "IfcBuildingElementProxyType" (IFCTEXT)
    IfcExportType = "USERDEFINED" (IFCTEXT)
  COBie | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetIdentifier = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    Category = "Pr_40_30_21_65:Plastics cycle lockers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black, Red, Yellow, Royal Blue, Light Blue, Dark Green, Light Green, Grey, Stone effect, Multicolour" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "The Minipod is a unique product designed to get children cycling. The Minipod is an innovative product which allows 8 bikes and 8 scooters to be secured" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10 year minimum" (IFCTEXT)
    Features = "Space saving, eco-friendly, secure, design" (IFCTEXT)
    Finish = "Dimpled effect finish" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    Manufacturer = "info@cyclepods.co.uk" (IFCTEXT)
    Material = "100% Recyclable MDPE plastic 100% Recyclable and 100% Recycled MDPE plastic (black)" (IFCTEXT)
    ModelNumber = "MINI001" (IFCTEXT)
    ModelReference = "Minipod" (IFCTEXT)
    Name = "PlasticsCycleLockers_Minipod_CyclepodsLtd" (IFCTEXT)
    NominalHeight = 1043.00000158536 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1409.00000214168 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1409.00000214168 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    Shape = "Circular" (IFCTEXT)
    Size = "1043 x 1409 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyDescription = "10 years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_40_30_21_65:Plastics cycle lockers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black, Red, Yellow, Royal Blue, Light Blue, Dark Green, Light Green, Grey, Stone effect, Multicolour" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "The Minipod is a unique product designed to get children cycling. The Minipod is an innovative product which allows 8 bikes and 8 scooters to be secured" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10 year minimum" (IFCTEXT)
    Features = "Space saving, eco-friendly, secure, design" (IFCTEXT)
    Finish = "Dimpled effect finish" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "info@cyclepods.co.uk" (IFCTEXT)
    Material = "100% Recyclable MDPE plastic 100% Recyclable and 100% Recycled MDPE plastic (black)" (IFCTEXT)
    ModelNumber = "MINI001" (IFCTEXT)
    ModelReference = "Minipod" (IFCTEXT)
    Name = "PlasticsCycleLockers_Minipod_CyclepodsLtd" (IFCTEXT)
    NominalHeight = 1043.00000158536 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 1409.00000214168 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 1409.00000214168 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Circular" (IFCTEXT)
    Size = "1043 x 1409 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "10 years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here", "London", "London", "United Kingdom"